Hamilton DTM Installation Guide

The packet "ArcSensorDTM_V1.2.0_Setup.msi" installs the following
components on Windows XP 32Bit and Windows 7 32Bit or 64Bit:
- ArcSensorDTM (for HDM [Hamilton Device Manager = separate installation])
- Pre-installation of the wireless converter driver
- Pre-installation of the USB-RS485 serial converter driver

Do not plugin any converters to the computer’s USB-port
until the software installation has finished.

For installation administrator rights on the PC are necessary.

1.  Unpack ZIP-file and run "ArcSensorDTM_V1.2.0_Setup.msi"

2.  Depending on your computer environment it may
    pop up a Windows-Message "Open File - Security Warning", click "Run"

3.  Welcome Screen: click "Next"

4.  License Agreement Screen: select "I accept" and click "Next"

5.  Installation Folder Screen: accept the default by clicking "Next"

6.  Ready to Install Screen: click "Install"

7.  Depending on the Windows-Security-Settings of your computer it may
    pop up a Windows-Message, in
    - Windows XP: "Software Installation", click "Continue Anyway"
    - Windows 7: "Windows Security", click "Install"

8.  Completing Screen: click "Finish"

9.  Plugin your converter to the computer’s USB-port
    - In case of a USB-RS485 Converter the driver is installed automatically
    - In case of a Wireless Converter
      > For Windows 7 the driver is installed automatically
      > For Windows XP follow the next steps

10. Found New Hardware Wizard: select “No, not this time” and click “Next”

11. Found New Hardware Wizard: select “Install the software automatically
    (Recommended)” and click “Next”

12. Depending on the Windows-Security-Settings of your computer it may
    pop up a Windows-Message "Hardware Installation", click "Continue Anyway"

13. Found New Hardware Wizard: click “Finish”
